LabView Driver Revision 3.0
___________________________
Powered by KOD Integrations
www.kodintegrations.com
___________________________

*************************************************
***** THIS DRIVER WILL REQUIRE LABVIEW 2014 *****
*************************************************

DESCRIPTION
This sample was designed specifically for interfacing with Arcus Technology's USB 2.0 communication products
using LabVIEW. 

*****************************************************
LabVIEW Driver Installation - Version 3.0
*****************************************************
Must be installed first (\\built\installers\arcus-usb-comm-installer\Volume\setup.exe) before any examples can 
be run, including the source code packaged with the DMX Application Note. 

*****************************************************
LabVIEW DMX-J-SA Application Note
*****************************************************
The documentation for the Arcus Technology LabVIEW driver by KOD Integrations. The app note will provide all the 
required details for using and understanding the Arcus Technology LabVIEW driver.

*****************************************************
LabVIEW DMX-J-SA Utility Panel Executable
*****************************************************
Will contain the executable of the DMX-J-SA Utility Panel. This executable works specifically with the DMX-J-SA USB 
motor. The executable allows for initial testing of the motor and its available operations. All executables require 
that LabVIEW 2014 Runtime be installed (http://www.ni.com/download/labview-run-time-engine-2014/4887/en/).  They do 
not require the LabVIEW development environment to be installed, nor do they require the LabVIEW Driver version 3.0 
be installed.

*****************************************************
LabVIEW PMX-4EX-SA Utility Panel Executable
*****************************************************
Will contain the executable of the PMX-4EX-SA Utility Panel. This executable works specifically with the PMX-4EX-SA
4-axis controller. The executable allows for initial testing of the motor and its available operations. All 
executables require that LabVIEW 2014 Runtime be installed (http://www.ni.com/download/labview-run-time-engine-2014/4887/en/).  
They do not require the LabVIEW development environment to be installed, nor do they require the LabVIEW Driver 
version 3.0 be installed.

*****************************************************
LabVIEW Console Panel Executable
*****************************************************
Will contain the executable of the simple temrinal Consol Panel. This executable allows the user to manually send 
ASCII commands to any Arcus Technology USB product. All executables require that LabVIEW 2014 Runtime be installed 
(http://www.ni.com/download/labview-run-time-engine-2014/4887/en/).  They do not require the LabVIEW development 
environment to be installed, nor do they require the LabVIEW Driver version 3.0 
be installed.